

**GOVERNMENT OF KHYBER PAKHTUNKHWA**

**PAKHTUNKHWA ENERGY DEVELOPMENT ORGANIZATION (PEDO)**

**NOTICE FOR Pre-Qualification/ Tender (Advance Action)**

Pakhtunkhwa Energy Development Organization (PEDO), invites applications from the Firms having experience in supply and operation of Rental Diesel Generator set of above 1 MW (documented proof be provided). PEDO intends to install 4.5 MW DG set (on rent basis) for supplying electricity to its consumers of Reshun HPP, district Chitral, for the period of 1 year; through its 33 KV transmission system.

2. Interested firm must submit the below proforma duly filled and supported by the documentary proof, otherwise their proposal/brushier will not be considered for evaluation.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PROFORMA FOR PRE-QUALIFICATION** | | | | | | | | |
| **Name of Firm** | **Pre-requisite** | | **Experience** | **Financial Soundness** | **Personnel** | | **Capacity of DG set the firm can provide** | **Fitness certificate of the available DG set** |
| **(Registrations)** | **List of Rental Projects** | **Completion certificate of similar completed projects** | **Bank Statement** | **Technical (operation) staff** | **Maintenance staff** |
|  | *Yes/No*  *Name:*  *Date of Regg:* | *Supply and operation of at least 2 projects, with capacity of 1 MW or above.* | *Max. 5 projects of supply and installation of DG set.* | *Last 3 years* | *No. of technical staff currently employed* | *Maintenance staff currently employed* | *List of DG sets (MVA) available with the firm.* | *Fitness certificate of the DG, if any, available with the firm.* |

After Pre-qualification, the Technical and Financial bids will be called with following considerations:

1. The DG set will be feeding three feeders of 33 KV transmission and distribution system.

2. The step up transformers available at site are 3 to 33 KV step-up (2MVA), so DG set voltage must be step-up.

3. Power of DG set must be synched /connected to common bus bar for transmission & dispatch.

4. No WAPDA/ PESCO supply is available at site; DG set be the only source of supply.

5. Proposed rented diesel generator is 4.5 MW (3X1.5MW units), with synchronization panel and other allied switch gear panels and accessories.

6. Installation, commission and testing, loading and unloading of the DG set be on Firms.

7. All operation and maintenance be the responsibility of firm.

8. Provision of Diesel for DG set will be according to agreed terms and conditions.

9. Quotation price must include transportation and all other applicable taxes.

10 The client PEDO (Pakhtunkhwa energy development organization) will prefer that the payment be based on per kilo-watt hour (per unit) basis.

11. The duration of operation of the DG set is suggested 6-8 Hours per day by the client.

12. Certificate of the fitness of proposed DG set be provided to the client.

The Proforma along with the supported documents should reach to the undersigned office in sealed envelopes before or on dated 14.2.2017 at 16:00 hrs. The successful pre-qualified firms will be announced on the official website and through letters and must apply for RFP/ TORS with in 10 days after the announcement of successful firms and subsequently the financial and technical bid will be invited from Pre-qualified firms. Further details/information can be obtained from the below mentioned office during working hours.

**PROJECT DIRECTOR RESHUN HPP , PEDO**

**ROOM # 223, PEDO HOUSE, 38/B-II PHASE-V**

**HAYATABAD PESHAWAR.**

**TEL # 091-9217360**